| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_drv_rtc_config_t Struct Reference
RTC driver

RTC driver instance configuration structure. More...

`#include <nrf_drv_rtc.h>`

## Data Fields
uint16_t | prescaler
uint8_t | interrupt_priority
uint8_t | tick_latency
bool | reliable

## Detailed Description

RTC driver instance configuration structure.

## Field Documentation

uint8_t nrf_drv_rtc_config_t::interrupt_priority

Interrupt priority.

uint16_t nrf_drv_rtc_config_t::prescaler

Prescaler.

bool nrf_drv_rtc_config_t::reliable

Reliable mode flag.

uint8_t nrf_drv_rtc_config_t::tick_latency

Maximum length of interrupt handler in ticks (max 7.7 ms).