| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_enable_params_t Struct Reference
Structures

BLE GAP initialization parameters. More...

`#include <ble_gap.h>`

## Data Fields
uint8_t | periph_conn_count
uint8_t | central_conn_count
uint8_t | central_sec_count
ble_gap_device_name_t const * | p_device_name

## Detailed Description

BLE GAP initialization parameters.

## Field Documentation

uint8_t ble_gap_enable_params_t::central_conn_count

Number of connections acting as a central

uint8_t ble_gap_enable_params_t::central_sec_count

Number of SMP instances for all connections acting as a central.

ble_gap_device_name_t const* ble_gap_enable_params_t::p_device_name

Pointer to device name instance. If NULL, sd_ble_enable() will set the device name to BLE_GAP_DEVNAME_DEFAULT.

uint8_t ble_gap_enable_params_t::periph_conn_count

Number of connections acting as a peripheral