| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_addr_t Struct Reference
Structures

Bluetooth Low Energy address. More...

`#include <ble_gap.h>`

## Data Fields
uint8_t | addr_id_peer: 1
uint8_t | addr_type: 7
uint8_t | addr [(6)]

## Detailed Description

Bluetooth Low Energy address.

## Field Documentation

uint8_t ble_gap_addr_t::addr[(6)]

48-bit address, LSB format.

uint8_t ble_gap_addr_t::addr_id_peer

        Only valid for peer addresses.

Reference to peer in device identities list (as set with sd_ble_gap_device_identities_set) when peer is using privacy.

uint8_t ble_gap_addr_t::addr_type

See GAP Address types.