| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Health Thermometer Service
This information applies to the following SoftDevices: S130, S132, S332

This module implements the Health Thermometer Service.

If an event handler is supplied by the application, the Health Thermometer Service will generate Health Thermometer Service events to the application.

Note
  The application must propagate BLE stack events to the Health Thermometer Service module by calling ble_hts_on_ble_evt() from the SoftDevice Event Handler function.