| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gatt_enable_params_t Struct Reference
Structures

BLE GATT initialization parameters. More...

`#include <ble_gatt.h>`

## Data Fields
uint16_t | att_mtu

## Detailed Description

BLE GATT initialization parameters.

## Field Documentation

uint16_t ble_gatt_enable_params_t::att_mtu

              Maximum size of ATT packet the SoftDevice can send or receive.

If it is 0 then GATT_MTU_SIZE_DEFAULT will be used. Otherwise GATT_MTU_SIZE_DEFAULT is the minimum value.

Relevant Message Sequence Charts

  GATTC ATT_MTU Exchange
  GATTS ATT_MTU Exchange