| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - a -

- acc : nrf_drv_qdec_report_data_evt_t
- accdbl : nrf_drv_qdec_report_data_evt_t
- accumulated_power : ant_bpwr_page16_data_t
- accumulated_torque : ant_bpwr_page_torque_data_t
- ack_resposne : ant_common_page70_data_t
- action : nrf_drv_gpiote_out_config_t , pm_peer_data_update_succeeded_evt_t , pm_peer_data_update_failed_t
- active_high : led_sb_init_params_t , low_power_pwm_config_t
- active_state : app_button_cfg_t
- addr : nrf_drv_twis_config_t
- address : nrf_drv_twi_xfer_desc_t
- advdata : ble_adv_init_t
- ain : nrf_drv_adc_channel_config_t
- alert : ble_ans_c_evt_t
- alert_category : ble_ans_alert_notification_t
- alert_category_count : ble_ans_alert_notification_t
- alert_level : ble_ias_evt_t , ble_ias_c_evt_t , ble_lls_evt_t
- alert_level_char : ble_ias_c_s
- alert_level_handles : ble_ias_s , ble_lls_s
- alert_msg_length : ble_ans_alert_notification_t
- alert_notif_ctrl_point : ble_ans_c_service_t
- alignment : nrf_drv_i2s_config_t
- analog_channel : nrf_drv_csense_evt_t
- ancs_attr_list : ble_ancs_c_t
- ans_email_support : ble_ans_alert_settings_t
- ans_high_prioritized_alert_support : ble_ans_alert_settings_t
- ans_instant_message_support : ble_ans_alert_settings_t
- ans_missed_call_support : ble_ans_alert_settings_t
- ans_news_support : ble_ans_alert_settings_t
- ans_notification_call_support : ble_ans_alert_settings_t
- ans_schedule_support : ble_ans_alert_settings_t
- ans_simple_alert_support : ble_ans_alert_settings_t
- ans_sms_mms_support : ble_ans_alert_settings_t
- ans_voice_mail_support : ble_ans_alert_settings_t
- ANT_PAGE70_RESPONSE_INVALID : ant_common_page70_data_t
- ANT_PAGE70_RESPONSE_TRANSMIT_UNTIL_SUCCESS : ant_common_page70_data_t
- app_version : nrf_dfu_settings_t
- attr : ble_ancs_c_evt_t
- attr_handle : nrf_ble_qwr_evt_t
- attr_handles : nrf_ble_qwr_t
- attr_id : ble_ancs_c_evt_notif_attr_t , ble_ancs_c_attr_list_t
- attr_len : ble_ancs_c_attr_list_t , ble_ancs_c_evt_notif_attr_t
- auth_code : nrf_ble_bms_ctrlpt_t , nrf_ble_bms_evt_t
- auth_status : nrf_ble_bms_s
- auto_change : ant_hrm_simulator_cb_t , ant_bsc_simulator_cb_t , ant_bpwr_simulator_cb_t , ant_sdm_simulator_cb_t
- auto_zero_status : ant_bpwr_page1_data_t
- aux_data_ref_count : nfc_ac_rec_payload_desc_t
- available_features : ble_lns_init_s , ble_lns_s , ble_lncp_s , ble_lncp_init_t