| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_lncp_init_t Struct Reference
Location and Navigation Service Control Point

## Data Fields
uint16_t | service_handle
ble_lncp_evt_handler_t | evt_handler
ble_srv_error_handler_t | error_handler
uint32_t | available_features
bool | is_position_quality_present
bool | is_control_point_present
bool | is_navigation_present
ble_gatts_char_handles_t | navigation_handles
uint32_t | total_distance
uint32_t | elevation
security_req_t | write_perm
security_req_t | cccd_write_perm

## Field Documentation

uint32_t ble_lncp_init_t::available_features

Value of the LN feature.

bool ble_lncp_init_t::is_control_point_present

If set to true, the control point characteristic will be added. Else not.

bool ble_lncp_init_t::is_navigation_present

If set to true, the navigation characteristic will be added. Else not.

bool ble_lncp_init_t::is_position_quality_present

If set to true, the position quality characteristic will be added. Else not.