| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ANT_TIME_SYNC_CONFIG Struct Reference
ANT Stack Parameters

Time synchronization configuration structure. More...

`#include <ant_parameters.h>`

## Data Fields
uint8_t | ucTimeBase
| Time base Time Base Defines.
bool | bInvalidationEnabled
| False: Invalidation is NOT used, True: Invalidation is used.
uint8_t | ucInvalidationByte
| The byte used to indicate an invalid time sync packet.

## Detailed Description

Time synchronization configuration structure.