| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
LPCOMP peripheral driver configuration
LPCOMP driver

## Macros
#define | LPCOMP_ENABLED
| Enable LPCOMP driver * Set to 1 to activate. More...
#define | LPCOMP_CONFIG_REFERENCE
| Reference voltage * Following options are avaiable: More...
#define | LPCOMP_CONFIG_DETECTION
| Detection * Following options are avaiable: More...
#define | LPCOMP_CONFIG_INPUT
| Analog input * Following options are avaiable: More...
#define | LPCOMP_CONFIG_IRQ_PRIORITY
| Interrupt priority. More...

## Detailed Description

## Macro Definition Documentation

#define LPCOMP_CONFIG_DETECTION

Detection * Following options are avaiable:

- 0 - Crossing
- 1 - Up
- 2 - Down

Note
  This is an NRF_CONFIG macro.

#define LPCOMP_CONFIG_INPUT

Analog input * Following options are avaiable:

- 0
- 1
- 2
- 3
- 4
- 5
- 6
- 7

Note
  This is an NRF_CONFIG macro.

#define LPCOMP_CONFIG_IRQ_PRIORITY

Interrupt priority.

Priorities 0,2 (nRF51) and 0,1,4,5 (nRF52) are reserved for SoftDevice

Following options are avaiable:

- 0 - 0 (highest)
- 1 - 1
- 2 - 2
- 3 - 3
- 4 - 4 (except nRF51 family)
- 5 - 5 (except nRF51 family)
- 6 - 6 (except nRF51 family)
- 7 - 7 (except nRF51 family)

Note
  This is an NRF_CONFIG macro.

#define LPCOMP_CONFIG_REFERENCE

Reference voltage * Following options are avaiable:

- 0 - Supply 1/8
- 1 - Supply 2/8
- 2 - Supply 3/8
- 3 - Supply 4/8
- 4 - Supply 5/8
- 5 - Supply 6/8
- 6 - Supply 7/8
- 8 - Supply 1/16 (nRF52)
- 9 - Supply 3/16 (nRF52)
- 10 - Supply 5/16 (nRF52)
- 11 - Supply 7/16 (nRF52)
- 12 - Supply 9/16 (nRF52)
- 13 - Supply 11/16 (nRF52)
- 14 - Supply 13/16 (nRF52)
- 15 - Supply 15/16 (nRF52)
- 7 - External Ref 0
- 65543 - External Ref 1

Note
  This is an NRF_CONFIG macro.

#define LPCOMP_ENABLED

Enable LPCOMP driver * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.