| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_evt_sec_info_request_t Struct Reference
Structures

Event structure for BLE_GAP_EVT_SEC_INFO_REQUEST. More...

`#include <ble_gap.h>`

## Data Fields
ble_gap_addr_t | peer_addr
ble_gap_master_id_t | master_id
uint8_t | enc_info: 1
uint8_t | id_info: 1
uint8_t | sign_info: 1

## Detailed Description

Event structure for BLE_GAP_EVT_SEC_INFO_REQUEST.

## Field Documentation

uint8_t ble_gap_evt_sec_info_request_t::enc_info

If 1, Encryption Information required.

uint8_t ble_gap_evt_sec_info_request_t::id_info

If 1, Identity Information required.

ble_gap_master_id_t ble_gap_evt_sec_info_request_t::master_id

Master Identification for LTK lookup.

ble_gap_addr_t ble_gap_evt_sec_info_request_t::peer_addr

Bluetooth address of the peer device.

uint8_t ble_gap_evt_sec_info_request_t::sign_info

If 1, Signing Information required.