| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gattc_handle_value_t Struct Reference
Structures

GATT read by UUID handle value pair. More...

`#include <ble_gattc.h>`

## Data Fields
uint16_t | handle
uint8_t * | p_value

## Detailed Description

GATT read by UUID handle value pair.

## Field Documentation

uint16_t ble_gattc_handle_value_t::handle

Attribute Handle.

uint8_t* ble_gattc_handle_value_t::p_value

Pointer to the Attribute Value, length is available in ble_gattc_evt_char_val_by_uuid_read_rsp_t::value_len.