| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_conn_sec_t Struct Reference
Structures

GAP connection security status. More...

`#include <ble_gap.h>`

## Data Fields
ble_gap_conn_sec_mode_t | sec_mode
uint8_t | encr_key_size

## Detailed Description

GAP connection security status.

## Field Documentation

uint8_t ble_gap_conn_sec_t::encr_key_size

Length of currently active encryption key, 7 to 16 octets (only applicable for bonding procedures).

ble_gap_conn_sec_mode_t ble_gap_conn_sec_t::sec_mode

Currently active security mode for this connection.