| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ant_channel_config_t Struct Reference
ANT channel configuration

ANT channel configuration structure. More...

`#include <ant_channel_config.h>`

## Data Fields
uint8_t | channel_number
| Assigned channel number.
uint8_t | channel_type
| Channel type (see Assign Channel Parameters in ant_parameters.h: ANT Stack Parameters).
uint8_t | ext_assign
| Extended assign (see Ext. Assign Channel Parameters in ant_parameters.h: ANT Stack Parameters).
uint8_t | rf_freq
| Radio frequency offset from 2400 MHz (for example, 2466 MHz, rf_freq = 66).
uint8_t | transmission_type
| Transmission type.
uint8_t | device_type
| Device type.
uint16_t | device_number
| Device number.
uint16_t | channel_period
| The period in 32 kHz counts.
uint8_t | network_number
| Network number denoting the network key.

## Detailed Description

ANT channel configuration structure.