| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
Assigned Values for BLE UUIDs
Defines

## Macros
#define | BLE_UUID_UNKNOWN 0x0000
#define | BLE_UUID_SERVICE_PRIMARY 0x2800
#define | BLE_UUID_SERVICE_SECONDARY 0x2801
#define | BLE_UUID_SERVICE_INCLUDE 0x2802
#define | BLE_UUID_CHARACTERISTIC 0x2803
#define | BLE_UUID_DESCRIPTOR_CHAR_EXT_PROP 0x2900
#define | BLE_UUID_DESCRIPTOR_CHAR_USER_DESC 0x2901
#define | BLE_UUID_DESCRIPTOR_CLIENT_CHAR_CONFIG 0x2902
#define | BLE_UUID_DESCRIPTOR_SERVER_CHAR_CONFIG 0x2903
#define | BLE_UUID_DESCRIPTOR_CHAR_PRESENTATION_FORMAT 0x2904
#define | BLE_UUID_DESCRIPTOR_CHAR_AGGREGATE_FORMAT 0x2905
#define | BLE_UUID_GATT 0x1801
#define | BLE_UUID_GATT_CHARACTERISTIC_SERVICE_CHANGED 0x2A05
#define | BLE_UUID_GAP 0x1800
#define | BLE_UUID_GAP_CHARACTERISTIC_DEVICE_NAME 0x2A00
#define | BLE_UUID_GAP_CHARACTERISTIC_APPEARANCE 0x2A01
#define | BLE_UUID_GAP_CHARACTERISTIC_PPF 0x2A02
#define | BLE_UUID_GAP_CHARACTERISTIC_RECONN_ADDR 0x2A03
#define | BLE_UUID_GAP_CHARACTERISTIC_PPCP 0x2A04

## Detailed Description

## Macro Definition Documentation

#define BLE_UUID_CHARACTERISTIC 0x2803

Characteristic.

#define BLE_UUID_DESCRIPTOR_CHAR_AGGREGATE_FORMAT 0x2905

Characteristic Aggregate Format Descriptor.

#define BLE_UUID_DESCRIPTOR_CHAR_EXT_PROP 0x2900

Characteristic Extended Properties Descriptor.

#define BLE_UUID_DESCRIPTOR_CHAR_PRESENTATION_FORMAT 0x2904

Characteristic Presentation Format Descriptor.

#define BLE_UUID_DESCRIPTOR_CHAR_USER_DESC 0x2901

Characteristic User Description Descriptor.

#define BLE_UUID_DESCRIPTOR_CLIENT_CHAR_CONFIG 0x2902

Client Characteristic Configuration Descriptor.

#define BLE_UUID_DESCRIPTOR_SERVER_CHAR_CONFIG 0x2903

Server Characteristic Configuration Descriptor.

#define BLE_UUID_GAP 0x1800

Generic Access Profile.

#define BLE_UUID_GAP_CHARACTERISTIC_APPEARANCE 0x2A01

Appearance Characteristic.

#define BLE_UUID_GAP_CHARACTERISTIC_DEVICE_NAME 0x2A00

Device Name Characteristic.

#define BLE_UUID_GAP_CHARACTERISTIC_PPCP 0x2A04

Peripheral Preferred Connection Parameters Characteristic.

#define BLE_UUID_GAP_CHARACTERISTIC_PPF 0x2A02

Peripheral Privacy Flag Characteristic.

#define BLE_UUID_GAP_CHARACTERISTIC_RECONN_ADDR 0x2A03

Reconnection Address Characteristic.

#define BLE_UUID_GATT 0x1801

Generic Attribute Profile.

#define BLE_UUID_GATT_CHARACTERISTIC_SERVICE_CHANGED 0x2A05

Service Changed Characteristic.

#define BLE_UUID_SERVICE_INCLUDE 0x2802

Include.

#define BLE_UUID_SERVICE_PRIMARY 0x2800

Primary Service.

#define BLE_UUID_SERVICE_SECONDARY 0x2801

Secondary Service.

#define BLE_UUID_UNKNOWN 0x0000

Reserved UUID.