| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
SPI/SPIM peripheral driver configuration
SPI master driver

## Macros
#define | SPI_ENABLED
| Set to 1 to activate. More...
#define | SPI_CONFIG_LOG_ENABLED
| Enables logging in the module. * Set to 1 to activate. More...
#define | SPI_CONFIG_LOG_LEVEL
| Default Severity level * Following options are avaiable: More...
#define | SPI_CONFIG_INFO_COLOR
| ANSI escape code prefix. * Following options are avaiable: More...
#define | SPI_CONFIG_DEBUG_COLOR
| ANSI escape code prefix. * Following options are avaiable: More...
#define | SPI_DEFAULT_CONFIG_IRQ_PRIORITY
| Interrupt priority. More...
#define | SPI0_ENABLED
| Enable SPI0 instance * Set to 1 to activate. More...
#define | SPI0_USE_EASY_DMA
| Use EasyDMA * Set to 1 to activate. More...
#define | SPI1_ENABLED
| Enable SPI1 instance * Set to 1 to activate. More...
#define | SPI1_USE_EASY_DMA
| Use EasyDMA * Set to 1 to activate. More...
#define | SPI2_ENABLED
| Enable SPI2 instance * Set to 1 to activate. More...
#define | SPI2_USE_EASY_DMA
| Use EasyDMA * Set to 1 to activate. More...

## Detailed Description

## Macro Definition Documentation

#define SPI0_ENABLED

Enable SPI0 instance * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define SPI0_USE_EASY_DMA

Use EasyDMA * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define SPI1_ENABLED

Enable SPI1 instance * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define SPI1_USE_EASY_DMA

Use EasyDMA * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define SPI2_ENABLED

Enable SPI2 instance * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define SPI2_USE_EASY_DMA

Use EasyDMA * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define SPI_CONFIG_DEBUG_COLOR

ANSI escape code prefix. * Following options are avaiable:

- 0 - Default
- 1 - Black
- 2 - Red
- 3 - Green
- 4 - Yellow
- 5 - Blue
- 6 - Magenta
- 7 - Cyan
- 8 - White

Note
  This is an NRF_CONFIG macro.

#define SPI_CONFIG_INFO_COLOR

ANSI escape code prefix. * Following options are avaiable:

- 0 - Default
- 1 - Black
- 2 - Red
- 3 - Green
- 4 - Yellow
- 5 - Blue
- 6 - Magenta
- 7 - Cyan
- 8 - White

Note
  This is an NRF_CONFIG macro.

#define SPI_CONFIG_LOG_ENABLED

Enables logging in the module. * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define SPI_CONFIG_LOG_LEVEL

Default Severity level * Following options are avaiable:

- 0 - Off
- 1 - Error
- 2 - Warning
- 3 - Info
- 4 - Debug

Note
  This is an NRF_CONFIG macro.

#define SPI_DEFAULT_CONFIG_IRQ_PRIORITY

Interrupt priority.

Priorities 0,2 (nRF51) and 0,1,4,5 (nRF52) are reserved for SoftDevice

Following options are avaiable:

- 0 - 0 (highest)
- 1 - 1
- 2 - 2
- 3 - 3
- 4 - 4 (except nRF51 family)
- 5 - 5 (except nRF51 family)
- 6 - 6 (except nRF51 family)
- 7 - 7 (except nRF51 family)

Note
  This is an NRF_CONFIG macro.

#define SPI_ENABLED

- Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.