| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
nrf_csense module configuration
Capacitive Sensor Library

## Macros
#define | NRF_CSENSE_ENABLED
| Enabling CSENSE capcitive touch sensor module * Set to 1 to activate. More...
#define | NRF_CSENSE_PAD_HYSTERESIS
| Minimal value of change to decide that pad was touched. *. More...
#define | NRF_CSENSE_PAD_DEVIATION
| Minimal value measured on pad to take its value while calculating step. *. More...
#define | NRF_CSENSE_MIN_PAD_VALUE
| Minimum normalized value on pad to take its value into account. *. More...
#define | NRF_CSENSE_MAX_PADS_NUMBER
| Maximum number of pads used for one instance. *. More...
#define | NRF_CSENSE_MAX_VALUE
| Maximum normalized value got from measurement. *. More...
#define | NRF_CSENSE_OUTPUT_PIN
| Output pin used by lower module. More...

## Detailed Description

## Macro Definition Documentation

#define NRF_CSENSE_ENABLED

Enabling CSENSE capcitive touch sensor module * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define NRF_CSENSE_MAX_PADS_NUMBER

Maximum number of pads used for one instance. *.

Note
  This is an NRF_CONFIG macro.

#define NRF_CSENSE_MAX_VALUE

Maximum normalized value got from measurement. *.

Note
  This is an NRF_CONFIG macro.

#define NRF_CSENSE_MIN_PAD_VALUE

Minimum normalized value on pad to take its value into account. *.

Note
  This is an NRF_CONFIG macro.

#define NRF_CSENSE_OUTPUT_PIN

Output pin used by lower module.

This is only used when running on NRF51.

Note
  This is an NRF_CONFIG macro.

#define NRF_CSENSE_PAD_DEVIATION

Minimal value measured on pad to take its value while calculating step. *.

Note
  This is an NRF_CONFIG macro.

#define NRF_CSENSE_PAD_HYSTERESIS

Minimal value of change to decide that pad was touched. *.

Note
  This is an NRF_CONFIG macro.