| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - c -

- cadence : ant_sdm_page2_data_t
- cadence_event_time : ant_bsc_combined_page0_data_t
- cadence_rev_count : ant_bsc_combined_page0_data_t
- cadence_sensorsim_cfg : ant_bpwr_simulator_cb_t
- cadence_sensorsim_state : ant_bpwr_simulator_cb_t
- cadence_sim_val : ant_bsc_simulator_cb_t
- cadency_is_valid : ant_sdm_page22_data_t
- calib_handler : ant_bpwr_sens_config_t
- calib_temp : nrf_ble_cgms_sensor_annunc_t
- calibration_id : ant_bpwr_page1_data_t
- calibration_val : ble_cgms_s
- callback : nrf_ble_qwr_t , nrf_ble_qwr_init_t , fs_config_t , app_twi_transaction_t
- calorie_is_valid : ant_sdm_page22_data_t
- calories : ant_sdm_page3_data_t
- carbohydrate : ble_gls_meas_context_t
- carbohydrate_id : ble_gls_meas_context_t
- carrier_data_ref : nfc_ac_rec_payload_desc_t
- category : ble_ans_control_point_t
- category_count : ble_ancs_c_evt_notif_t
- category_id : ble_ancs_c_evt_notif_t
- cc : type_2_tag_t
- cc_channel_count : nrf_drv_rtc_t , nrf_drv_timer_t
- cccd_handle : ble_gatt_db_char_t
- cccd_write_access : ble_add_char_params_t
- cccd_write_perm : ble_srv_cccd_security_mode_t
- central_handle : ble_ans_c_s
- cgms_com_state : ble_cgms_s
- channel : nrf_drv_saadc_limit_evt_t , ant_evt_t
- channel_0 : nrf_pwm_values_individual_t , nrf_pwm_values_wave_form_t
- channel_1 : nrf_pwm_values_individual_t , nrf_pwm_values_wave_form_t
- channel_2 : nrf_pwm_values_individual_t , nrf_pwm_values_wave_form_t
- channel_3 : nrf_pwm_values_individual_t
- channel_number : ant_channel_config_t , ant_bpwr_profile_s , ant_bsc_profile_s , ant_hrm_profile_s , ant_sdm_profile_s , ant_search_config_t
- channel_period : ant_channel_config_t
- channel_type : ant_channel_config_t
- channels : nrf_drv_i2s_config_t
- char_count : ble_gatt_db_srv_t
- char_ext_props : ble_add_char_params_t
- char_handles : ble_cts_c_evt_t , ble_cts_c_s , ble_hids_rep_char_t , ble_cgms_s
- char_id : ble_hids_evt_t
- char_props : ble_add_char_user_desc_t , ble_add_char_params_t
- characteristic : ble_gatt_db_char_t
- charateristics : ble_gatt_db_srv_t
- check_byte_0 : type_2_tag_serial_number_t
- check_byte_1 : type_2_tag_serial_number_t
- clear_bus_init : nrf_drv_twi_config_t
- client_serial_number : antfs_params_t
- clock_freq : nrf_drv_pdm_config_t
- close_func : nrf_dfu_transport_t
- coarse_bat_volt : ant_bsc_page4_data_t
- code : nrf_ble_bms_auth_code_t
- comm_interval : ble_cgms_s
- command : ble_ans_control_point_t
- command_crc : dfu_progress_t
- command_offset : dfu_progress_t
- command_size : dfu_progress_t
- command_type : ant_common_page70_data_t
- common : ant_bpwr_profile_s , ant_sdm_profile_s
- company_identifier : ble_advdata_manuf_data_t
- computed_heart_rate : ant_hrm_page0_data_t
- config : nrf_drv_adc_channel_s
- conn_handle : ble_sc_ctrlpt_s , ble_hids_s , ble_gls_s , ble_bas_c_evt_t , ble_db_discovery_t , ble_db_discovery_evt_t , ble_ancs_c_evt_t , ble_ancs_c_t , ble_ans_c_evt_t , ble_ans_c_s , ble_bas_s , ble_cgms_s , ble_bas_c_s , ble_bps_s , ble_cscs_s , ble_cts_c_evt_t , ble_cts_c_s , pm_evt_t , ble_rscs_c_s , ble_hrs_s , ble_hrs_c_evt_t , ble_lbs_c_s , ble_hrs_c_s , nrf_ble_bms_s , ble_ias_s , ble_rscs_s , ble_ias_c_evt_t , ble_lls_s , ble_ias_c_s , ble_nus_s , ble_rscs_c_evt_t , ble_lbs_c_evt_t , ble_nus_c_s , ble_lbs_s , ble_tps_t , ble_lns_s , nrf_ble_qwr_t , ble_hts_s
- conn_sec_failed : pm_evt_t
- conn_sec_succeeded : pm_evt_t
- connected : pm_conn_sec_status_t
- context : ble_gls_rec_t
- control_point_char : ble_dfu_s , ble_ancs_c_service_t
- count_mode : nrf_drv_pwm_config_t
- counter_top : nrf_pwm_values_wave_form_t
- cps : nfc_ac_rec_payload_desc_t
- crc : nrf_dfu_res_t , nrf_dfu_settings_t , antfs_event_return_t , nrf_esb_config_t
- crc16 : fds_ic_t
- csc_ctrlpt_attr_md : ble_cscs_init_t
- csc_feature_attr_md : ble_cscs_init_t
- csc_meas_attr_md : ble_cscs_init_t
- csc_sensor_loc_attr_md : ble_cscs_init_t
- csn_pin : nrf_drv_spis_config_t
- csn_pullup : nrf_drv_spis_config_t
- ctrl_point_security_req_cccd_write_perm : ble_dfu_init_t , ble_lns_init_s
- ctrl_point_security_req_write_perm : ble_lns_init_s , ble_dfu_init_t
- ctrl_pt : ble_cscs_s
- ctrlpt_evt_handler : ble_cscs_init_t
- ctrlpt_handles : nrf_ble_bms_s
- ctrplt_supported_functions : ble_cscs_init_t
- cts_cccd_handle : ble_cts_c_handles_t
- cts_handle : ble_cts_c_handles_t
- cts_pin_no : app_uart_comm_params_t
- cumulative_crank_revs : ble_cscs_meas_s
- cumulative_time : ant_bsc_simulator_cb_t
- cumulative_time_frac : ant_bsc_simulator_cb_t
- cumulative_wheel_revs : ble_cscs_meas_s
- curr_char_ind : ble_db_discovery_t
- curr_srv_ind : ble_db_discovery_t
- current_attr_index : ble_ancs_c_t
- current_time : ble_cts_c_evt_t
- current_transfer_idx : app_twi_t
- current_val : sensorsim_state_t