| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
SLIP protocol implementation used by HCI configuration
SLIP module

## Macros
#define | HCI_SLIP_ENABLED
| Enabling HCI transport module. * Set to 1 to activate. More...
#define | HCI_UART_BAUDRATE
| Default Baudrate * Following options are avaiable: More...
#define | HCI_UART_FLOW_CONTROL
| Hardware Flow Control * Following options are avaiable: More...
#define | HCI_UART_RX_PIN
| UART RX pin *. More...
#define | HCI_UART_TX_PIN
| UART TX pin *. More...
#define | HCI_UART_RTS_PIN
| UART RTS pin *. More...
#define | HCI_UART_CTS_PIN
| UART CTS pin *. More...

## Detailed Description

## Macro Definition Documentation

#define HCI_SLIP_ENABLED

Enabling HCI transport module. * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define HCI_UART_BAUDRATE

Default Baudrate * Following options are avaiable:

- 323584 - 1200 baud
- 643072 - 2400 baud
- 1290240 - 4800 baud
- 2576384 - 9600 baud
- 3862528 - 14400 baud
- 5152768 - 19200 baud
- 7716864 - 28800 baud
- 10289152 - 38400 baud
- 15400960 - 57600 baud
- 20615168 - 76800 baud
- 30801920 - 115200 baud (nRF52 family only)
- 30924800 - 115200 baud (nRF51 family only)
- 61865984 - 230400 baud
- 67108864 - 250000 baud
- 121634816 - 460800 baud
- 251658240 - 921600 baud
- 268435456 - 57600 baud

Note
  This is an NRF_CONFIG macro.

#define HCI_UART_CTS_PIN

UART CTS pin *.

Note
  This is an NRF_CONFIG macro.

#define HCI_UART_FLOW_CONTROL

Hardware Flow Control * Following options are avaiable:

- 0 - Disabled
- 1 - Enabled

Note
  This is an NRF_CONFIG macro.

#define HCI_UART_RTS_PIN

UART RTS pin *.

Note
  This is an NRF_CONFIG macro.

#define HCI_UART_RX_PIN

UART RX pin *.

Note
  This is an NRF_CONFIG macro.

#define HCI_UART_TX_PIN

UART TX pin *.

Note
  This is an NRF_CONFIG macro.