| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_addr_t Struct Reference
Structures

Bluetooth Low Energy address. More...

`#include <ble_gap.h>`

## Data Fields
uint8_t | addr_type
uint8_t | addr [6]

## Detailed Description

Bluetooth Low Energy address.

## Field Documentation

uint8_t ble_gap_addr_t::addr[6]

48-bit address, LSB format.

uint8_t ble_gap_addr_t::addr_type

See GAP Address types.