| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_evt_lesc_dhkey_request_t Struct Reference
Structures

Event structure for BLE_GAP_EVT_LESC_DHKEY_REQUEST. More...

`#include <ble_gap.h>`

## Data Fields
ble_gap_lesc_p256_pk_t * | p_pk_peer
uint8_t | oobd_req:1

## Detailed Description

Event structure for BLE_GAP_EVT_LESC_DHKEY_REQUEST.

## Field Documentation

uint8_t ble_gap_evt_lesc_dhkey_request_t::oobd_req

LESC OOB data required. A call to sd_ble_gap_lesc_oob_data_set is required to complete the procedure.

ble_gap_lesc_p256_pk_t* ble_gap_evt_lesc_dhkey_request_t::p_pk_peer

     LE Secure Connections remote P-256 Public Key. This will point to the application-supplied memory

inside the keyset during the call to sd_ble_gap_sec_params_reply.