| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ulong_union_t Union Reference
ANT-FS client device simulator

uint32_t type presentation as an union. More...

`#include <defines.h>`

## Data Fields
uint32_t | data
uint8_t | data_bytes [sizeof(uint32_t)]
struct {
uint8_t byte0
uint8_t byte1
uint8_t byte2
uint8_t byte3
} | bytes

## Detailed Description

uint32_t type presentation as an union.

## Field Documentation

uint8_t ulong_union_t::byte0

Byte 0 of the data content.

uint8_t ulong_union_t::byte1

Byte 1 of the data content.

uint8_t ulong_union_t::byte2

Byte 2 of the data content.

uint8_t ulong_union_t::byte3

Byte 3 of the data content.

uint32_t ulong_union_t::data

The data content as a single variable.

uint8_t ulong_union_t::data_bytes[sizeof(uint32_t)]

The data content as a byte array.