| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_bas_init_t Struct Reference
Battery Service

Battery Service init structure. This contains all options and data needed for initialization of the service. More...

`#include <ble_bas.h>`

## Data Fields
ble_bas_evt_handler_t | evt_handler
bool | support_notification
ble_srv_report_ref_t * | p_report_ref
uint8_t | initial_batt_level
ble_srv_cccd_security_mode_t | battery_level_char_attr_md
ble_gap_conn_sec_mode_t | battery_level_report_read_perm

## Detailed Description

Battery Service init structure. This contains all options and data needed for initialization of the service.

## Field Documentation

ble_srv_cccd_security_mode_t ble_bas_init_t::battery_level_char_attr_md

Initial security level for battery characteristics attribute

ble_gap_conn_sec_mode_t ble_bas_init_t::battery_level_report_read_perm

Initial security level for battery report read attribute

ble_bas_evt_handler_t ble_bas_init_t::evt_handler

Event handler to be called for handling events in the Battery Service.

uint8_t ble_bas_init_t::initial_batt_level

Initial battery level

ble_srv_report_ref_t* ble_bas_init_t::p_report_ref

If not NULL, a Report Reference descriptor with the specified value will be added to the Battery Level characteristic

bool ble_bas_init_t::support_notification

TRUE if notification of Battery Level measurement is supported.