| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Modules
Proprietary stacks

Application Programming Interface for proprietary protocols. More...

## Modules
| Enhanced ShockBurst
| Enhanced ShockBurst (ESB) is a basic protocol that supports two-way data packet communication including packet buffering, packet acknowledgment, and automatic retransmission of lost packets.
| Gazell Link Layer
| nRF51 only: Gazell Link Layer Application Programming Interface (API).
| Gazell Pairing
| nRF51 only: Gazell Pairing API.

## Detailed Description

Application Programming Interface for proprietary protocols.