| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Enumerations
Enumerations
Master Boot Record API

## Enumerations
enum | NRF_MBR_SVCS { SD_MBR_COMMAND = (0x18) }
| nRF Master Boot Record API SVC numbers. More...
enum | NRF_MBR_COMMANDS { SD_MBR_COMMAND_COPY_BL, SD_MBR_COMMAND_COPY_SD, SD_MBR_COMMAND_INIT_SD, SD_MBR_COMMAND_COMPARE, SD_MBR_COMMAND_VECTOR_TABLE_BASE_SET }
| Possible values for sd_mbr_command_t.command. More...

## Detailed Description

## Enumeration Type Documentation

enum NRF_MBR_COMMANDS

Possible values for sd_mbr_command_t.command.

Enumerator
SD_MBR_COMMAND_COPY_BL | Copy a new BootLoader. See Also sd_mbr_command_copy_bl_t
SD_MBR_COMMAND_COPY_SD | Copy a new SoftDevice. See Also sd_mbr_command_copy_sd_t
SD_MBR_COMMAND_INIT_SD | Init forwarding interrupts to SD, and run reset function in SD
SD_MBR_COMMAND_COMPARE | This command works like memcmp. See Also sd_mbr_command_compare_t
SD_MBR_COMMAND_VECTOR_TABLE_BASE_SET | Start forwarding all exception to this address See Also sd_mbr_command_vector_table_base_set_t

enum NRF_MBR_SVCS

nRF Master Boot Record API SVC numbers.

Enumerator
SD_MBR_COMMAND | sd_mbr_command