| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - m -

- main_mode : nrf_drv_comp_config_t
- main_page_number : ant_bsc_sens_config_t , ant_hrm_sens_config_t
- major_version : nfc_hs_rec_payload_desc_t , type_2_tag_capability_container_t
- mantissa : ieee_float32_t , ieee_float16_t , sfloat_t
- manuf_id : ant_bsc_page2_data_t , ant_hrm_page2_data_t
- manuf_spec : ant_hrm_page4_data_t
- manufact_name_str : ble_dis_init_t
- manufacturer_id : ble_dis_sys_id_t , ant_common_page80_data_t , type_2_tag_serial_number_t
- max : sensorsim_cfg_t
- max_aux_data_ref : nfc_ac_rec_payload_desc_t
- max_burst_block_size : antfs_request_info_t
- max_conn_interval : ble_advdata_conn_int_t
- max_conn_params_update_count : ble_conn_params_init_t
- max_file_size : antfs_request_info_t
- max_len : ble_hids_inp_rep_init_t , ble_hids_outp_rep_init_t , ble_hids_feature_rep_init_t , ble_add_char_params_t , ble_add_descr_params_t
- max_record_count : nfc_ndef_msg_desc_t
- max_size : ble_add_char_user_desc_t , nrf_dfu_res_t
- max_tlv_blocks : type_2_tag_t
- mck_pin : nrf_drv_i2s_config_t
- mck_setup : nrf_drv_i2s_config_t
- meal : ble_gls_meas_context_t
- mean_arterial_pressure : ble_bps_meas_s
- meas : ble_gls_rec_t , ble_cgms_rec_t
- meas_handles : ble_hts_s , ble_bps_s , ble_cscs_s , ble_rscs_s
- measurement_status : ble_bps_meas_s
- measurement_status_present : ble_bps_meas_s
- measurment : nrf_ble_cgms_char_handler_t
- medication : ble_gls_meas_context_t
- medication_id : ble_gls_meas_context_t
- mem_buffer : nrf_ble_qwr_t , nrf_ble_qwr_init_t
- message : ble_error_log_data_t
- message_buffer_size : ble_ans_c_s , ble_ans_c_init_t
- min : sensorsim_cfg_t
- min_conn_interval : ble_advdata_conn_int_t
- minor_version : type_2_tag_capability_container_t , nfc_hs_rec_payload_desc_t
- miso_drive : nrf_drv_spis_config_t
- miso_pin : nrf_drv_spis_config_t , nrf_drv_spi_config_t
- mitm_protected : pm_conn_sec_status_t
- mode : nrf_esb_config_t , nrf_drv_spi_config_t , nrf_drv_spis_config_t , nrf_drv_timer_config_t , nrf_drv_i2s_config_t , ant_encrypt_channel_settings_t , nrf_drv_pdm_config_t
- model_num : ant_bsc_page3_data_t , ant_hrm_page3_data_t
- model_num_str : ble_dis_init_t
- model_number : ant_common_page80_data_t
- mosi_pin : nrf_drv_spi_config_t , nrf_drv_spis_config_t