| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
Types of UUID
Defines

## Macros
#define | BLE_UUID_TYPE_UNKNOWN 0x00
#define | BLE_UUID_TYPE_BLE 0x01
#define | BLE_UUID_TYPE_VENDOR_BEGIN 0x02

## Detailed Description

## Macro Definition Documentation

#define BLE_UUID_TYPE_BLE 0x01

Bluetooth SIG UUID (16-bit).

#define BLE_UUID_TYPE_UNKNOWN 0x00

Invalid UUID type.

#define BLE_UUID_TYPE_VENDOR_BEGIN 0x02

Vendor UUID types start at this index (128-bit).