| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_hrs_init_t Struct Reference
Heart Rate Service

Heart Rate Service init structure. This contains all options and data needed for initialization of the service. More...

`#include <ble_hrs.h>`

## Data Fields
ble_hrs_evt_handler_t | evt_handler
bool | is_sensor_contact_supported
uint8_t * | p_body_sensor_location
ble_srv_cccd_security_mode_t | hrs_hrm_attr_md
ble_srv_security_mode_t | hrs_bsl_attr_md

## Detailed Description

Heart Rate Service init structure. This contains all options and data needed for initialization of the service.

## Field Documentation

ble_hrs_evt_handler_t ble_hrs_init_t::evt_handler

Event handler to be called for handling events in the Heart Rate Service.

ble_srv_security_mode_t ble_hrs_init_t::hrs_bsl_attr_md

Initial security level for body sensor location attribute

ble_srv_cccd_security_mode_t ble_hrs_init_t::hrs_hrm_attr_md

Initial security level for heart rate service measurement attribute

bool ble_hrs_init_t::is_sensor_contact_supported

Determines if sensor contact detection is to be supported.

uint8_t* ble_hrs_init_t::p_body_sensor_location

If not NULL, initial value of the Body Sensor Location characteristic.