| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_rscs_init_t Struct Reference
Running Speed and Cadence Service

Running Speed and Cadence Service init structure. This contains all options and data needed for initialization of the service. More...

`#include <ble_rscs.h>`

## Data Fields
ble_rscs_evt_handler_t | evt_handler
ble_srv_cccd_security_mode_t | rsc_meas_attr_md
ble_srv_security_mode_t | rsc_feature_attr_md
uint16_t | feature
ble_rscs_meas_t | initial_rcm

## Detailed Description

Running Speed and Cadence Service init structure. This contains all options and data needed for initialization of the service.

## Field Documentation

ble_rscs_evt_handler_t ble_rscs_init_t::evt_handler

Event handler to be called for handling events in the Running Speed and Cadence Service.

uint16_t ble_rscs_init_t::feature

Initial value for features of sensor.

ble_rscs_meas_t ble_rscs_init_t::initial_rcm

Initial Running Speed Cadence Measurement.

ble_srv_security_mode_t ble_rscs_init_t::rsc_feature_attr_md

Initial security level for feature attribute

ble_srv_cccd_security_mode_t ble_rscs_init_t::rsc_meas_attr_md

Initial security level for running speed and cadence measurement attribute