| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
fds_record_chunk_t Struct Reference
Flash Data Storage

A chunk of record data to be written to flash. More...

`#include <fds.h>`

## Data Fields
void const * | p_data
| Pointer to the data to store. Must be word-aligned.
uint16_t | length_words
| Length of data pointed to by `p_data` (in 4-byte words).

## Detailed Description

A chunk of record data to be written to flash.

`p_data` must be aligned to a word boundary. Make sure to keep it in memory until the operation has completed, which is indicated by the respective FDS event.