| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_enable_params_t Struct Reference
Structures

BLE GAP initialization parameters. More...

`#include <ble_gap.h>`

## Data Fields
uint8_t | periph_conn_count
uint8_t | central_conn_count
uint8_t | central_sec_count

## Detailed Description

BLE GAP initialization parameters.

## Field Documentation

uint8_t ble_gap_enable_params_t::central_conn_count

Number of connections acting as a central

uint8_t ble_gap_enable_params_t::central_sec_count

Number of SMP instances for all connections acting as a central.

uint8_t ble_gap_enable_params_t::periph_conn_count

Number of connections acting as a peripheral