| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages

### - i -

- ic : fds_header_t
- ic_revision : nrf_ic_info_t
- id : fs_evt_t , fds_evt_t
- id_length : nfc_ndef_record_desc_t
- image_crc : nrf_dfu_bank_t
- image_size : nrf_dfu_bank_t
- important : ble_ancs_c_notif_flags_t
- include_appearance : ble_advdata_t
- include_ble_device_addr : ble_advdata_t
- included_services_count : ble_hids_init_t
- incr : sensorsim_cfg_t
- info : ant_encrypt_stack_settings_t
- init_command : nrf_dfu_settings_t
- init_func : nrf_dfu_transport_t
- init_len : ble_add_char_params_t , ble_add_descr_params_t
- init_offs : ble_add_descr_params_t
- init_state : nrf_drv_gpiote_out_config_t
- initial_alert_level : ble_lls_init_t
- initial_batt_level : ble_bas_init_t
- initial_rcm : ble_rscs_init_t
- initial_run_time : nrf_ble_cgms_init_t
- initial_sensor_status : nrf_ble_cgms_init_t
- initial_tx_power_level : ble_tps_init_t
- initialized : nrf_ble_qwr_t
- inp_rep_array : ble_hids_s
- inp_rep_count : ble_hids_init_t , ble_hids_s
- input : nrf_drv_lpcomp_config_t , nrf_drv_adc_channel_config_t , nrf_drv_comp_config_t
- inst_cadence : ble_rscs_meas_s , ble_rsc_t
- inst_speed : ble_rscs_meas_s , ble_rsc_t
- inst_stride_length : ble_rscs_meas_s , ble_rsc_t
- instance_id : nrf_drv_rtc_t , nrf_drv_spis_t , nrf_drv_timer_t
- instant_speed : ble_lns_loc_speed_s
- instant_speed_present : ble_lns_loc_speed_s
- instantaneous_cadence : ant_bpwr_common_data_t
- instantaneous_power : ant_bpwr_page16_data_t
- instNr : nrf_drv_twis_t
- internal : type_2_tag_serial_number_t
- internal_transaction_in_progress : app_twi_t
- internal_transaction_result : app_twi_t
- interrupt_priority : nrf_drv_adc_config_t , nrf_drv_comp_config_t , nrf_drv_lpcomp_config_t , nrf_drv_pdm_config_t , nrf_drv_qdec_config_t , nrf_drv_rng_config_t , nrf_drv_rtc_config_t , nrf_drv_saadc_config_t , nrf_drv_timer_config_t , nrf_drv_twi_config_t , nrf_drv_twis_config_t , nrf_drv_uart_config_t , nrf_drv_wdt_config_t
- irq : nrf_drv_spi_t , nrf_drv_spis_t , nrf_drv_rtc_t
- irq_priority : nrf_drv_i2s_config_t , nrf_drv_pwm_config_t , nrf_drv_spi_config_t , nrf_drv_spis_config_t
- is_context_supported : ble_gls_init_t
- is_control_point_present : ble_lncp_s , ble_lns_init_s , ble_lncp_init_t
- is_crank_rev_data_present : ble_cscs_meas_s
- is_ctrlpt_indication_enabled : ble_lncp_s
- is_data_available : antfs_beacon_status_byte1_t
- is_defered_read : ble_add_char_user_desc_t , ble_add_char_params_t , ble_add_descr_params_t
- is_defered_write : ble_add_char_user_desc_t , ble_add_char_params_t , ble_add_descr_params_t
- is_expended_energy_supported : ble_hrs_s
- is_increasing : sensorsim_state_t
- is_inst_stride_len_present : ble_rsc_t , ble_rscs_meas_s
- is_kb : ble_hids_init_t
- is_loc_speed_notification_enabled : ble_lns_s
- is_mouse : ble_hids_init_t
- is_nav_notification_enabled : ble_lns_s , ble_lncp_s
- is_navigation_present : ble_lncp_init_t , ble_lncp_s , ble_lns_init_s , ble_lns_s
- is_navigation_running : ble_lncp_s
- is_notification_enabled : ble_nus_s
- is_notification_supported : ble_bas_s
- is_pairing_enabled : antfs_beacon_status_byte1_t
- is_position_quality_present : ble_lns_init_s , ble_lncp_init_t , ble_lncp_s
- is_running : ble_rsc_t , ble_rscs_meas_s
- is_sensor_contact_detected : ble_hrs_s
- is_sensor_contact_supported : ble_hrs_s , ble_hrs_init_t
- is_session_started : ble_cgms_s
- is_total_distance_present : ble_rsc_t , ble_rscs_meas_s
- is_upload_enabled : antfs_beacon_status_byte1_t
- is_user_mem_reply_pending : nrf_ble_qwr_t
- is_value_user : ble_add_descr_params_t , ble_add_char_user_desc_t , ble_add_char_params_t
- is_var_len : ble_add_char_user_desc_t , ble_add_descr_params_t , ble_add_char_params_t
- is_watcher : nrf_drv_gpiote_in_config_t
- is_wheel_rev_data_present : ble_cscs_meas_s
- isource : nrf_drv_comp_config_t
- item_sz : app_mailbox_t