| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_ias_c_s Struct Reference
Immediate Alert Service Client

IAS Client structure. This contains various status information for the client. More...

`#include <ble_ias_c.h>`

## Data Fields
ble_ias_c_evt_handler_t | evt_handler
ble_srv_error_handler_t | error_handler
uint16_t | conn_handle
ble_uuid_t | service_uuid
ble_gattc_char_t | alert_level_char

## Detailed Description

IAS Client structure. This contains various status information for the client.

## Field Documentation

ble_gattc_char_t ble_ias_c_s::alert_level_char

IAS Alert Level Characteristic. Stores data about the alert characteristic found on the peer.

uint16_t ble_ias_c_s::conn_handle

Handle of the current connection. Set with ble_ias_c_handles_assign when connected.

ble_srv_error_handler_t ble_ias_c_s::error_handler

Function to be called in case of an error.

ble_ias_c_evt_handler_t ble_ias_c_s::evt_handler

Event handler to be called for handling events in the Immediate Alert Service client.

ble_uuid_t ble_ias_c_s::service_uuid

The GATT Service holding the discovered Immediate Service.