| S212 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - _ -

- __cr_flag : nrf_nvic_state_t
- __irq_masks : nrf_nvic_state_t

### - a -

- address : sd_mbr_command_vector_table_base_set_t

### - b -

- bActiveState : ANT_PA_LNA_CONFIG
- base_set : sd_mbr_command_t
- bEnable : ANT_HIGH_DUTY_SEARCH_CONFIG
- bEnabled : ANT_PA_LNA_CONFIG
- bInvalidationEnabled : ANT_TIME_SYNC_CONFIG
- bl_len : sd_mbr_command_copy_bl_t
- bl_src : sd_mbr_command_copy_bl_t
- bTimeStampEnabled : ANT_TIME_STAMP_CONFIG

### - c -

- callback_action : nrf_radio_signal_callback_return_param_t
- ciphertext : nrf_ecb_hal_data_t
- cleartext : nrf_ecb_hal_data_t
- command : sd_mbr_command_t
- compare : sd_mbr_command_t
- copy_bl : sd_mbr_command_t
- copy_sd : sd_mbr_command_t

### - d -

- distance_us : nrf_radio_request_normal_t
- dst : sd_mbr_command_copy_sd_t

### - e -

- earliest : nrf_radio_request_t
- extend : nrf_radio_signal_callback_return_param_t

### - h -

- hfclk : nrf_radio_request_earliest_t , nrf_radio_request_normal_t

### - k -

- key : nrf_ecb_hal_data_t

### - l -

- len : sd_mbr_command_copy_sd_t , sd_mbr_command_compare_t
- length_us : nrf_radio_request_normal_t , nrf_radio_request_earliest_t , nrf_radio_signal_callback_return_param_t

### - n -

- normal : nrf_radio_request_t

### - p -

- p_ciphertext : nrf_ecb_hal_data_block_t
- p_cleartext : nrf_ecb_hal_data_block_t
- p_key : nrf_ecb_hal_data_block_t
- p_next : nrf_radio_signal_callback_return_param_t
- params : nrf_radio_request_t , nrf_radio_signal_callback_return_param_t
- priority : nrf_radio_request_earliest_t , nrf_radio_request_normal_t
- ptr1 : sd_mbr_command_compare_t
- ptr2 : sd_mbr_command_compare_t

### - r -

- rc_ctiv : nrf_clock_lf_cfg_t
- rc_temp_ctiv : nrf_clock_lf_cfg_t
- request : nrf_radio_signal_callback_return_param_t
- request_type : nrf_radio_request_t

### - s -

- source : nrf_clock_lf_cfg_t
- src : sd_mbr_command_copy_sd_t

### - t -

- timeout_us : nrf_radio_request_earliest_t

### - u -

- ucGPIO : ANT_PA_LNA_CONFIG
- ucGPIOTECh : ANT_PA_LNA_CONFIG
- ucInvalidationByte : ANT_TIME_SYNC_CONFIG
- ucPPIChDisable : ANT_PA_LNA_CONFIG
- ucPPIChEnable : ANT_PA_LNA_CONFIG
- ucSearchSuppressionWindows : ANT_HIGH_DUTY_SEARCH_CONFIG
- ucTimeBase : ANT_TIME_SYNC_CONFIG , ANT_TIME_STAMP_CONFIG
- usRestartInterval : ANT_HIGH_DUTY_SEARCH_CONFIG

### - x -

- xtal_accuracy : nrf_clock_lf_cfg_t