| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_ancs_c_attr_list_t Struct Reference
Apple Notification Service client

iOS notification attribute content wanted by our application. More...

`#include <ble_ancs_c.h>`

## Data Fields
bool | get
ble_ancs_c_notif_attr_id_values_t | attr_id
uint16_t | attr_len
uint8_t * | p_attr_data

## Detailed Description

iOS notification attribute content wanted by our application.

## Field Documentation

ble_ancs_c_notif_attr_id_values_t ble_ancs_c_attr_list_t::attr_id

Attribute ID: AppIdentifier(0), Title(1), Subtitle(2), Message(3), MessageSize(4), Date(5), PositiveActionLabel(6), NegativeActionLabel(7).

uint16_t ble_ancs_c_attr_list_t::attr_len

Length of the attribute. If more data is received from the Notification Provider, all data beyond this length is discarded.

bool ble_ancs_c_attr_list_t::get

Boolean to determine if this attribute will be requested from the Notification Provider.

uint8_t* ble_ancs_c_attr_list_t::p_attr_data

Pointer to where the memory is allocated for storing incoming attributes.