| S212 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ANT_PA_LNA_CONFIG Struct Reference
ANT Stack Parameters

The structure that holds configuration for PA/LNA GPIO outputs during radio events. More...

`#include <ant_parameters.h>`

## Data Fields
struct {
bool bEnabled
| Indicates that PA pin toggling is enabled.
uint8_t ucGPIO
| Selects the GPIO used to control the PA.
bool bActiveState
| Active state. 1 - Active high, 0 - Active low.
} | PA_CONFIG
struct {
bool bEnabled
| Indicates that LNA pin toggling is enabled.
uint8_t ucGPIO
| Selects the GPIO used to control the LNA.
bool bActiveState
| Active state. 1 - Active high, 0 - Active low.
} | LNA_CONFIG
uint8_t | ucGPIOTECh
| GPIOTE channel used to control PA and LNA pins.
uint8_t | ucPPIChEnable
| PPI channel used to control the PA/LNA signal before EVENTS_READY. Must be different from ucPPIChDisable.
uint8_t | ucPPIChDisable
| PPI channel used to control the PA/LNA signal during EVENTS_DISABLED. Must be different from ucPPIChEnable.

## Detailed Description

The structure that holds configuration for PA/LNA GPIO outputs during radio events.

## Field Documentation

bool ANT_PA_LNA_CONFIG::bEnabled

Indicates that PA pin toggling is enabled.

Indicates that LNA pin toggling is enabled.

uint8_t ANT_PA_LNA_CONFIG::ucGPIO

Selects the GPIO used to control the PA.

Selects the GPIO used to control the LNA.