| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_tps_init_t Struct Reference
TX Power Service

TX Power Service init structure. This contains all options and data needed for initialization of the service. More...

`#include <ble_tps.h>`

## Data Fields
int8_t | initial_tx_power_level
ble_srv_security_mode_t | tps_attr_md

## Detailed Description

TX Power Service init structure. This contains all options and data needed for initialization of the service.

## Field Documentation

int8_t ble_tps_init_t::initial_tx_power_level

Initial value of the TX Power Level characteristic (in dBm).

ble_srv_security_mode_t ble_tps_init_t::tps_attr_md

Initial Security Setting for TX Power Service Characteristics.