| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages

### - b -

- b_country_code : ble_hids_hid_information_t
- bank_0 : nrf_dfu_settings_t
- bank_1 : nrf_dfu_settings_t
- bank_code : nrf_dfu_bank_t
- bank_current : nrf_dfu_settings_t
- bank_layout : nrf_dfu_settings_t
- bas_db : ble_bas_c_evt_t
- base_clock : nrf_drv_pwm_config_t
- base_time : ble_gls_meas_t
- bat_status : ant_bsc_page4_data_t
- battery : ant_sdm_page2_data_t
- battery_level : ble_bas_c_evt_t
- battery_level_char_attr_md : ble_bas_init_t
- battery_level_handles : ble_bas_s
- battery_level_last : ble_bas_s
- battery_level_report_read_perm : ble_bas_init_t
- baud_rate : app_uart_comm_params_t
- baudrate : nrf_drv_uart_config_t
- bcd_hid : ble_hids_hid_information_t
- beacon_device_manufacturing_id : antfs_params_t
- beacon_device_type : antfs_params_t
- beacon_frequency : antfs_params_t
- beacon_status_byte1 : antfs_params_t
- bearing : ble_lns_navigation_s
- beat_count : ant_hrm_page0_data_t
- beat_time : ant_hrm_page0_data_t
- behaviour : nrf_drv_wdt_config_t
- bit_mask : low_power_pwm_config_t
- bit_order : nrf_drv_spi_config_t , nrf_drv_spis_config_t
- bit_width : nrf_drv_timer_config_t
- bitrate : nrf_esb_config_t
- bl_cccd_handle : ble_bas_c_db_t
- bl_handle : ble_bas_c_db_t
- ble_adv_directed_enabled : ble_adv_modes_config_t
- ble_adv_directed_slow_enabled : ble_adv_modes_config_t
- ble_adv_directed_slow_interval : ble_adv_modes_config_t
- ble_adv_directed_slow_timeout : ble_adv_modes_config_t
- ble_adv_fast_enabled : ble_adv_modes_config_t
- ble_adv_fast_interval : ble_adv_modes_config_t
- ble_adv_fast_timeout : ble_adv_modes_config_t
- ble_adv_slow_enabled : ble_adv_modes_config_t
- ble_adv_slow_interval : ble_adv_modes_config_t
- ble_adv_slow_timeout : ble_adv_modes_config_t
- ble_adv_whitelist_enabled : ble_adv_modes_config_t
- blood_pressure_diastolic : ble_bps_meas_s
- blood_pressure_systolic : ble_bps_meas_s
- blood_pressure_units_in_kpa : ble_bps_meas_s
- bms_ctrlpt_sec_req : nrf_ble_bms_init_t
- bms_feature_sec_req : nrf_ble_bms_init_t
- bond_callbacks : nrf_ble_bms_s , nrf_ble_bms_init_t
- bonded : pm_conn_sec_status_t
- boot_kb_inp_rep_handles : ble_hids_s
- boot_kb_outp_rep_handles : ble_hids_s
- boot_mouse_inp_rep_handles : ble_hids_s
- bootloader_version : nrf_dfu_settings_t
- bps_feature_attr_md : ble_bps_init_t
- bps_meas_attr_md : ble_bps_init_t
- bsl_handles : ble_hrs_s
- buf_req : nrf_drv_twis_evt_t
- buf_size_mask : app_fifo_t
- buffer_a : nrf_drv_pdm_config_t
- buffer_b : nrf_drv_pdm_config_t
- buffer_length : nrf_drv_pdm_config_t
- burn_rate : ant_sdm_simulator_cb_t , ant_sdm_simulator_cfg_t
- button : ble_lbs_c_evt_t
- button_cccd_handle : lbs_db_t
- button_char_handles : ble_lbs_s
- button_handle : lbs_db_t
- button_handler : app_button_cfg_t
- button_state : ble_button_t
- byte0 : ulong_union_t
- byte1 : ulong_union_t
- byte2 : ulong_union_t
- byte3 : ulong_union_t
- bytes : antfs_event_return_t , nrf_drv_uart_xfer_evt_t