| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_hids_inp_rep_init_t Struct Reference
Human Interface Device Service

HID Service Input Report characteristic init structure. This contains all options and data needed for initialization of one Input Report characteristic. More...

`#include <ble_hids.h>`

## Data Fields
uint16_t | max_len
ble_srv_report_ref_t | rep_ref
ble_srv_cccd_security_mode_t | security_mode
uint8_t | read_resp: 1

## Detailed Description

HID Service Input Report characteristic init structure. This contains all options and data needed for initialization of one Input Report characteristic.

## Field Documentation

uint16_t ble_hids_inp_rep_init_t::max_len

Maximum length of characteristic value.

uint8_t ble_hids_inp_rep_init_t::read_resp

Should application generate a response to read requests.

ble_srv_report_ref_t ble_hids_inp_rep_init_t::rep_ref

Value of the Report Reference descriptor.

ble_srv_cccd_security_mode_t ble_hids_inp_rep_init_t::security_mode

Security mode for the HID Input Report characteristic, including cccd.