| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gls_s Struct Reference
Glucose Service

Glucose Service structure. This contains various status information for the service. More...

`#include <ble_gls.h>`

## Data Fields
ble_gls_evt_handler_t | evt_handler
ble_srv_error_handler_t | error_handler
uint16_t | service_handle
ble_gatts_char_handles_t | glm_handles
ble_gatts_char_handles_t | glm_context_handles
ble_gatts_char_handles_t | glf_handles
ble_gatts_char_handles_t | racp_handles
uint16_t | conn_handle
uint16_t | feature
bool | is_context_supported

## Detailed Description

Glucose Service structure. This contains various status information for the service.

## Field Documentation

uint16_t ble_gls_s::conn_handle

Handle of the current connection (as provided by the BLE stack, is BLE_CONN_HANDLE_INVALID if not in a connection).

ble_srv_error_handler_t ble_gls_s::error_handler

Function to be called in case of an error.

ble_gls_evt_handler_t ble_gls_s::evt_handler

Event handler to be called for handling events in the Glucose Service.

ble_gatts_char_handles_t ble_gls_s::glf_handles

Handles related to the Glucose Feature characteristic.

ble_gatts_char_handles_t ble_gls_s::glm_context_handles

Handles related to the Glucose Measurement Context characteristic.

ble_gatts_char_handles_t ble_gls_s::glm_handles

Handles related to the Glucose Measurement characteristic.

ble_gatts_char_handles_t ble_gls_s::racp_handles

Handles related to the Record Access Control Point characteristic.

uint16_t ble_gls_s::service_handle

Handle of Glucose Service (as provided by the BLE stack).