| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Typedefs | Functions
Radio Notification Event Handler
BLE libraries

Module for propagating Radio Notification events to the application. More...

## Typedefs
typedef void(* | ble_radio_notification_evt_handler_t )(bool radio_active)
| Application radio notification event handler type.

## Functions
uint32_t | ble_radio_notification_init (uint32_t irq_priority, uint8_t distance, ble_radio_notification_evt_handler_t evt_handler)
| Function for initializing the Radio Notification module. More...

## Detailed Description

Module for propagating Radio Notification events to the application.

## Function Documentation

uint32_t ble_radio_notification_init | ( | uint32_t | irq_priority,
|  | uint8_t | distance,
|  | ble_radio_notification_evt_handler_t | evt_handler
| ) |  |

Function for initializing the Radio Notification module.

Parameters

  [in] | irq_priority | Interrupt priority for the Radio Notification interrupt handler.
  [in] | distance | The time from an Active event until the radio is activated.
  [in] | evt_handler | Handler to be executed when a radio notification event has been received.

Returns
  NRF_SUCCESS on successful initialization, otherwise an error code.