| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_pa_lna_cfg_t Struct Reference
Structures

Configuration parameters for the PA and LNA. More...

`#include <ble.h>`

## Data Fields
uint8_t | enable:1
uint8_t | active_high:1
uint8_t | gpio_pin:6

## Detailed Description

Configuration parameters for the PA and LNA.

## Field Documentation

uint8_t ble_pa_lna_cfg_t::active_high

Set the pin to be active high

uint8_t ble_pa_lna_cfg_t::enable

Enable toggling for this amplifier

uint8_t ble_pa_lna_cfg_t::gpio_pin

The GPIO pin to toggle for this amplifier