| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_ble_cgms_racp_t Struct Reference
Structures

Record Access Control Point transaction data. More...

`#include <nrf_ble_cgms.h>`

## Data Fields
uint8_t | racp_proc_operator
uint8_t | racp_proc_record_ndx
uint8_t | racp_proc_records_reported
uint8_t | racp_proc_records_reported_since_txcomplete
ble_racp_value_t | pending_racp_response
uint8_t | pending_racp_response_operand [2]

## Detailed Description

Record Access Control Point transaction data.

## Field Documentation

ble_racp_value_t nrf_ble_cgms_racp_t::pending_racp_response

RACP response to be sent.

uint8_t nrf_ble_cgms_racp_t::pending_racp_response_operand[2]

Operand of the RACP response to be sent.

uint8_t nrf_ble_cgms_racp_t::racp_proc_operator

Operator of the current request.

uint8_t nrf_ble_cgms_racp_t::racp_proc_record_ndx

Current record index.

uint8_t nrf_ble_cgms_racp_t::racp_proc_records_reported

Number of reported records.

uint8_t nrf_ble_cgms_racp_t::racp_proc_records_reported_since_txcomplete

Number of reported records since the last TX_COMPLETE event.