| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
app_uart_comm_params_t Struct Reference
UART module

UART communication structure holding configuration settings for the peripheral. More...

`#include <app_uart.h>`

## Data Fields
uint32_t | rx_pin_no
uint32_t | tx_pin_no
uint32_t | rts_pin_no
uint32_t | cts_pin_no
app_uart_flow_control_t | flow_control
bool | use_parity
uint32_t | baud_rate

## Detailed Description

UART communication structure holding configuration settings for the peripheral.

## Field Documentation

uint32_t app_uart_comm_params_t::baud_rate

Baud rate configuration.

uint32_t app_uart_comm_params_t::cts_pin_no

CTS pin number, only used if flow control is enabled.

app_uart_flow_control_t app_uart_comm_params_t::flow_control

Flow control setting, if flow control is used, the system will use low power UART mode, based on CTS signal.

uint32_t app_uart_comm_params_t::rts_pin_no

RTS pin number, only used if flow control is enabled.

uint32_t app_uart_comm_params_t::rx_pin_no

RX pin number.

uint32_t app_uart_comm_params_t::tx_pin_no

TX pin number.

bool app_uart_comm_params_t::use_parity

Even parity if TRUE, no parity if FALSE.