| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
TIMER periperal driver configuration
Timer driver

## Macros
#define | TIMER_ENABLED
| Set to 1 to activate. More...
#define | TIMER_DEFAULT_CONFIG_FREQUENCY
| Timer frequency if in Timer mode * Following options are avaiable: More...
#define | TIMER_DEFAULT_CONFIG_MODE
| Timer mode or operation * Following options are avaiable: More...
#define | TIMER_DEFAULT_CONFIG_BIT_WIDTH
| Timer counter bit width * Following options are avaiable: More...
#define | TIMER_DEFAULT_CONFIG_IRQ_PRIORITY
| Interrupt priority. More...
#define | TIMER0_ENABLED
| Enable TIMER0 instance * Set to 1 to activate. More...
#define | TIMER1_ENABLED
| Enable TIMER1 instance * Set to 1 to activate. More...
#define | TIMER2_ENABLED
| Enable TIMER2 instance * Set to 1 to activate. More...
#define | TIMER3_ENABLED
| Enable TIMER3 instance * Set to 1 to activate. More...
#define | TIMER4_ENABLED
| Enable TIMER4 instance * Set to 1 to activate. More...

## Detailed Description

## Macro Definition Documentation

#define TIMER0_ENABLED

Enable TIMER0 instance * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define TIMER1_ENABLED

Enable TIMER1 instance * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define TIMER2_ENABLED

Enable TIMER2 instance * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define TIMER3_ENABLED

Enable TIMER3 instance * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define TIMER4_ENABLED

Enable TIMER4 instance * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define TIMER_DEFAULT_CONFIG_BIT_WIDTH

Timer counter bit width * Following options are avaiable:

- 0 - 16 bit
- 1 - 8 bit
- 2 - 24 bit
- 3 - 32 bit

Note
  This is an NRF_CONFIG macro.

#define TIMER_DEFAULT_CONFIG_FREQUENCY

Timer frequency if in Timer mode * Following options are avaiable:

- 0 - 16 MHz
- 1 - 8 MHz
- 2 - 4 MHz
- 3 - 2 MHz
- 4 - 1 MHz
- 5 - 500 kHz
- 6 - 250 kHz
- 7 - 125 kHz
- 8 - 62.5 kHz
- 9 - 31.25 kHz

Note
  This is an NRF_CONFIG macro.

#define TIMER_DEFAULT_CONFIG_IRQ_PRIORITY

Interrupt priority.

Priorities 0,2 (nRF51) and 0,1,4,5 (nRF52) are reserved for SoftDevice

Following options are avaiable:

- 0 - 0 (highest)
- 1 - 1
- 2 - 2
- 3 - 3
- 4 - 4 (except nRF51 family)
- 5 - 5 (except nRF51 family)
- 6 - 6 (except nRF51 family)
- 7 - 7 (except nRF51 family)

Note
  This is an NRF_CONFIG macro.

#define TIMER_DEFAULT_CONFIG_MODE

Timer mode or operation * Following options are avaiable:

- 0 - Timer
- 1 - Counter

Note
  This is an NRF_CONFIG macro.

#define TIMER_ENABLED

- Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.