| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Advertising types
Defines

## Macros
#define | BLE_GAP_ADV_TYPE_ADV_IND 0x00
#define | BLE_GAP_ADV_TYPE_ADV_DIRECT_IND 0x01
#define | BLE_GAP_ADV_TYPE_ADV_SCAN_IND 0x02
#define | BLE_GAP_ADV_TYPE_ADV_NONCONN_IND 0x03

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_ADV_TYPE_ADV_DIRECT_IND 0x01

Connectable directed.

#define BLE_GAP_ADV_TYPE_ADV_IND 0x00

Connectable undirected.

#define BLE_GAP_ADV_TYPE_ADV_NONCONN_IND 0x03

Non connectable undirected.

#define BLE_GAP_ADV_TYPE_ADV_SCAN_IND 0x02

Scannable undirected.