| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Blinky RTX Example

The Blinky RTX Example shows RTX features like osSignal, osDelay, and osTimer.

When the application starts, two GPIO pins are configured as outputs using the BSP module to drive the LEDs. Then, a new thread and timer are created.

# Setup

You can find the source code and the project file of the example in the following folder: `<InstallFolder>\examples\peripheral\blinky_rtx`

LED assignments:

- LED 1 and LED 2: Blinking.

# Testing

Test the Blinky RTX Example application by performing the following steps:

1. Compile and program the application.
2. Observe that the LEDs are blinking.

Note
  See RTX support for more information about RTX.