| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Structures | Enumerations | Functions
IC information
SDK common libraries

Library for checking IC information (IC revision, RAM size, FLASH size). More...

## Data Structures
struct | nrf_ic_info_t
| IC information struct containing the IC revision, RAM size, and FLASH size. More...

## Enumerations
enum | nrf_ic_revision_t { IC_PART_UNKNOWN = 0, IC_REVISION_NRF51_REV1, IC_REVISION_NRF51_REV2, IC_REVISION_NRF51_REV3, IC_REVISION_NRF51_UNKNOWN }
| Enum identifying the IC revision as described in the Compatibility Matrix. More...

## Functions
void | nrf_ic_info_get (nrf_ic_info_t *p_ic_info)
| Function for returning information about the IC revision, the RAM size, and the FLASH size. More...

## Detailed Description

Library for checking IC information (IC revision, RAM size, FLASH size).

## Enumeration Type Documentation

enum nrf_ic_revision_t

Enum identifying the IC revision as described in the Compatibility Matrix.

Enumerator
IC_PART_UNKNOWN | IC Revision unknown.
IC_REVISION_NRF51_REV1 | IC Revision 1.
IC_REVISION_NRF51_REV2 | IC Revision 2.
IC_REVISION_NRF51_REV3 | IC Revision 3.
IC_REVISION_NRF51_UNKNOWN | IC Revision unknown.

## Function Documentation

void nrf_ic_info_get | ( | nrf_ic_info_t * | p_ic_info | ) |

Function for returning information about the IC revision, the RAM size, and the FLASH size.

Parameters

  [out] | p_ic_info | Struct containing IC revision, RAM size, and FLASH size.