| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_device_name_t Struct Reference
Structures

Device name and its properties. More...

`#include <ble_gap.h>`

## Data Fields
ble_gap_conn_sec_mode_t | write_perm
uint8_t | vloc:2
uint8_t * | p_value
uint16_t | current_len
uint16_t | max_len

## Detailed Description

Device name and its properties.

Note
  If max_len is more than BLE_GAP_DEVNAME_DEFAULT_LEN and vloc is set to BLE_GATTS_VLOC_STACK, the attribute table size must be increased to have room for the longer device name (see ble_gatts_enable_params_t).

## Field Documentation

uint16_t ble_gap_device_name_t::current_len

Current length in bytes of the memory pointed to by p_value.

uint16_t ble_gap_device_name_t::max_len

Maximum length in bytes of the memory pointed to by p_value.

uint8_t* ble_gap_device_name_t::p_value

Pointer to where the value (device name) is stored or will be stored.

uint8_t ble_gap_device_name_t::vloc

Value location, see GATT Value Locations.

ble_gap_conn_sec_mode_t ble_gap_device_name_t::write_perm

Write permissions.