| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_common_enable_params_t Struct Reference
Structures

BLE Common Initialization parameters. More...

`#include <ble.h>`

## Data Fields
uint16_t | vs_uuid_count
ble_conn_bw_counts_t * | p_conn_bw_counts

## Detailed Description

BLE Common Initialization parameters.

Note
  If p_conn_bw_counts is NULL the SoftDevice will assume default bandwidth configuration for all connections. To fit a custom bandwidth configuration requirement, the application developer may have to specify a custom memory pool configuration here. See ble_common_opt_conn_bw_t for bandwidth configuration of individual connections. Please refer to the SoftDevice Specification for more information on bandwidth configuration.

## Field Documentation

ble_conn_bw_counts_t* ble_common_enable_params_t::p_conn_bw_counts

Bandwidth configuration parameters or NULL for defaults.

uint16_t ble_common_enable_params_t::vs_uuid_count

Maximum number of 128-bit, Vendor Specific UUID bases to allocate.