| S212 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
sd_mbr_command_t Struct Reference
Types

## Data Fields
uint32_t | command
union {
sd_mbr_command_copy_sd_t copy_sd
sd_mbr_command_compare_t compare
sd_mbr_command_copy_bl_t copy_bl
sd_mbr_command_vector_table_base_set_t base_set
} | params

## Field Documentation

sd_mbr_command_vector_table_base_set_t sd_mbr_command_t::base_set

Parameters for vector table base set. Requires parameter page.

uint32_t sd_mbr_command_t::command

type of command to be issued see NRF_MBR_COMMANDS.

sd_mbr_command_compare_t sd_mbr_command_t::compare

Parameters for verify.

sd_mbr_command_copy_bl_t sd_mbr_command_t::copy_bl

Parameters for copy BootLoader. Requires parameter page.

sd_mbr_command_copy_sd_t sd_mbr_command_t::copy_sd

Parameters for copy SoftDevice.